BITS ER-Suite |
| Bedeutung der 'Maßeinheit' Codes (QuantityCodes)
| Auszug aus der Norm UNECERec20
| https://docs.peppol.eu/poacc/billing/3.0/2024-Q2/codelist/UNECERec20
| oder
| http://www.robert-kuhlemann.de/iso_masseinheiten.htm
Kurzzeichen |  | Deutsch | (English)
_3B | = |  | (megajoule)
_4G | = |  | (microlitre)
_4N | = |  | (megabecquerel)
_59 | = |  | (part per million)
AB | = |  | (Bulk pack)
ANN | = | Jahr | ()
BQL | = |  | (becquerel)
C26 | = |  | (millisecond)
C62, PCE | = | Stück [Stk] | (Piece)
CEL | = |  | (degree Celsius)
CEN | = |  | (Hundred)
CGM | = | Zentigramm | (centigram)
CLF | = | 100 Blätter | (hundred leave)
CLT | = |  | (centilitre)
CMK | = | [cm^2] | (square centimetre)
CMQ | = | [cm^3] | (cubic centimetre)
CMT | = | Zentimeter [cm] | ()
CNP | = |  | (hundred pack)
CTM | = | Metric Carat | ()
CUR | = |  | (curie)
D46 | = |  | (volt - ampere)
DAY | = | Tag | ()
DLT | = |  | (decilitre)
DMK | = |  | (square decimetre)
DMQ | = |  | (cubic decimetre)
DMT | = |  | (decimetre)
DTN | = | Zentner | ()
E48 | = |  | (Service)
EA | = |  | (each)
FF | = | Ar | (100 m^2)
FH | = |  | (micromole)
GRM | = | Gramm [gr] | ()
GV | = |  | (gigajoule)
H18, HAR | = |  | (square hectometre)
H87 | = | Stück [Stk] | (Piece)
HLT | = |  | (hectolitre)
HUR | = | Stunde [h] | ()
IE | = |  | (person)
K1 | = |  | (kilowatt)
K3 | = |  | (kilovolt)
K40 | = |  | (standard acceleration of free fall)
KGM | =[kg] | Kilogramm | ()
KJO | = |  | (kilojoule)
KMT, KTM | = | Kilometer [km] | ()
KT | = | Kit | ()
KVR | = |  | (kilovar)
KWH | = | Kilowattstunde | ()
KWT | = | Kilowatt | ()
L94 | = |  | (ton-force (US short))
LS | = |  | (Pauschale Abkürzung)
LTR | = | Liter [l] | ()
LUX | = |  | (lux)
M5 | = |  | (microcurie)
MAH | = |  | (megavolt ampere reactive hour)
MAW | = |  | (megawatt)
MBR | = |  | (millibar)
MC | = | Mikrogramm | (microgram)
MCU | = |  | (millicurie)
MGM | = | Milligramm | ()
MIN | = | Minute [min] | ()
MKD | = |  | (Square Metre Day)
MKM | = |  | (Square Metre Month)
MKW | = |  | (Square Metre Week)
MLT | = | Milliliter | ()
MMK | = | Quadratmillimeter [mm^2] | ()
MMQ | = | [mm^3] | (cubic millimetre)
MMT | = | Millimeter [mm] | ()
MON | = | Monat | ()
MQD | = |  | (Cubic Metre Day)
MQH | = |  | (cubic metre per hour)
MQM | = |  | (Cubic Metre Month)
MQS | = |  | (cubic metre per second)
MQW | = |  | (Cubic Metre Week)
MTK | = | Quadratmeter [m^2] | ()
MTQ | = | Kubikmeter [m^3] | ()
MTR | = | Meter [m] | ()
MTS | = | Meter pro Sekunde | ()
MWH | = | Megawatt Stunde | ()
NAR | = | Anzahl Artikel | ()
NMP | = |  | (number of packs)
P1 | = | Prozent [%] | ()
PR | = | Paar | ()
PTN | = |  | (Portion)
QAN | = | Quartal | ()
SAN | = | Halbjahr | ()
SEC | = | Sekunde [sec] | ()
SET | = |  | (Set)
T3 | = | Tausend Stück | ()
TNE | = | Tonne [t] | ()
TP | = |  | (Ten pack)
WEE | = | Woche | ()
X8A | = |  | (Pallet, wooden)
XAM | = |  | (Ampoule, non-protected)
XAP | = |  | (Ampoule, protected)
XBA | = | Fass | ()
XBC | = | Kiste oder Gestell | ()
XBD | = | Tafel | (Board)
XBE | = | Bündel | ()
XBF | = | Balloon | ()
XBG | = | Beutel | ()
XBJ | = | Eimer | ()
XBK | = | Korb | ()
XBO | = | Flasche | ()
XBX | = | Box | ()
XCA | = |  | (Can)
XCH | = | Container | ()
XCI | = | Kanister | ()
XCK | = |  | (Cask)
XCQ | = |  | (Cartridge Package)
XCR | = | Kiste | ()
XCS | = |  | (Case)
XCT | = | Karton | ()
XCU | = | Becher | ()
XCW | = |  | (Cage, roll)
XCX | = |  | (Can)
XDC | = |  | (Crate, multiple layer)
XDR | = | Trommel | ()
XFL | = |  | (Flask)
XGR | = |  | (Receptacle)
XMS | = |  | (Sack, multi-wall)
XMT | = | Matte | ()
XNE | = |  | ()
XOK, D64 | = | Block | ()
XOU | = |  | (Container)
XPA | = | Packet | ()
XPK | = | Verpackung Standard | ()
XPO | = |  | (Pouch)
XPP | = | Stück [Stk] | (Piece)
XPT | = |  | (Pot)
XPU | = |  | (Tray)
XPX | = | Palette | ()
XRD | = | Stange | ()
XRO | = | Rolle | ()
XSA | = | Sack | ()
XST | = | Bogen (Papier) | ()
XTN | = | Dose | ()
XTU | = | Tube | ()
Z9 | = |  | (nanomole)
ZZ | = |  | (Mutually Defined)